**Wall-mounted liquid soap dispenser, 1 litre**

Liquid soap or hydroalcoholic gel dispenser

Soft-touch, bright polished 304 stainless steel

Reference: **510580**

Specification description

Wall-mounted soap dispenser with soft-touch operation.

Liquid soap or hydroalcoholic gel dispenser.

Vandal-resistant model with lock and standard DELABIE key.

One-piece (monobloc) hinged cover for easy maintenance and improved hygiene.

Push-button with soft-touch operation: suitable for all users, people with reduced mobility, disabled, children, etc.

Anti-blocking: single dose per press, even if the button is pressed for prolonged periods.

No waste, non-drip (waterproof) pump dispenser.

Tank with large opening: easy to refill from large containers.

Tank prevents long-term stagnation of soap.

Window for monitoring soap level.

304 stainless steel, bright polished finish.

Stainless steel thickness: 1mm.

Capacity: 1 litre.

Dimensions: 90 x 105 x 252mm.

For vegetable-based liquid soap with a maximum viscosity of 3,000 mPa.s.

Compatible with hydroalcoholic gel.

Wall-mounted soap dispenser with 30-year warranty.