**Comfort shower seat to hang on grab bars**

Shower seat to hang on grab bars

UltraPolish bright polished stainless steel

Reference: **510300**

Specification description

Removable, hanging shower seat.

Shower seat for disabled people or for people with reduced mobility.

HR Comfort shower seat and backrest.

Large model.

Shower seat to hang on Ø 32mm grab bars (see refs. 5481P, 5120P2 and 50505P2).

Anti-bacterial treatment on seat and backrest: optimal protection against bacterial development and mould.

Removable: reduces the number of shower seats in a facility, allowing installation only when required e.g. hotels or hospitals providing short-term accommodation for people with reduced mobility.

Suitable for intensive use in public places or the healthcare sector.

Removable solid seat made from high-resistant polymer.

Uniform non-porous surface for easy maintenance and hygiene.

Withstands chemical products (Betadine®) and cleaning.

Anti-UV treatment.

Warm to the touch.

Bacteriostatic 304 stainless steel structure Ø 32mm.

UltraPolish bright polished structure.

Adjustable screw jacks guarantee a good horizontal position.

Large protective caps prevent damage to the wall.

Dimensions: 590 x 420 x 510mm.

Tested to over 200kg. Maximum recommended user weight: 135kg.

Removable shower seat with 30-year warranty. CE marked.