**ECO flow straightener**

Pre-set at 3 lpm

F22/100

Reference: **922022.2P**

Specification description

Scale resistant flow straightener pre-set at 3 lpm (DELABIE patented).

 Adjustable flow rate from 1.5 to 6 lpm at 3 bar (depending on the mixer/tap model) from the outside with a 2.5mm Allen key.

Flow straightener with no grid: reduces bacterial development (no water retention or scale deposits).

F22/100.

Supplied in packs of 2.

30-year warranty.The Water savings generated by the ECO flow straightener surpass the requirements of class 'Z' of the European standard EN 246.