**Stainless steel drop-down rail, satin, L. 650mm**

UltraSatin polished satin stainless steel

Ø 32mm

Reference: **510160S**

Specification description

Drop-down grab bar Ø 32mm, for people with reduced mobility.

Drop-down grab bar for WCs or showers.

Allows side access in the raised position.

In the lowered position use as a grab bar, for standing up and assisting movement.

Retained in upright position. Slowed down descent.

Drop-down grab bar made from bacteriostatic 304 stainless steel tube.

Stainless steel with UltraSatin polished satin finish, non-porous uniform surface for easy maintenance and hygiene.

Concealed fixings secured by a 4mm thick 304 stainless steel plate.

Supplied with stainless steel screws for concrete walls.

Dimensions: 650 x 230 x 105mm.

Tested to over 200kg. Maximum recommended user weight 135kg.

30-year warranty.

CE marked.