**Comfort backrest for WCs**

UltraSatin polished satin stainless steel structure

Black polyurethane

Reference: **510629S**

Specification description

Comfort backrest for WCs for people with reduced mobility.

Structure made from UltraSatin polished satin 304 bacteriostatic stainless steel.

Backrest for toilets made from soft polyurethane.

Tube Ø 25mm x 1.2mm.

Fixings concealed by a 3-hole cover plate, 304 stainless steel, Ø 72mm.

304 stainless steel cover plate.

Dimensions: 150 x 580 x 173mm.

30-year warranty. CE marked.