**White NylonClean anti-bacterial Nylon fixed support rail, L. 650mm**

Bright white anti-bacterial HR Nylon

Ø 32mm

Reference: **5161N**

Specification description

Wall support rail for people with reduced material.

Bright white HR Nylon.

Can be used as a grab bar and fixed support bar for WCs, showers or washbasins.

Generally installed parallel to a drop-down support bar in a WC or on either side of a washbasin.

Recommended if the WC pan or shower seat is a long way from the side wall.

Anti-bacterial NylonClean treatment: optimal protection against bacterial development.

Suitable for intensive use in public places or the healthcare sector.

High-strength polyamide (Nylon) and polymer: with 2mm reinforced steel core treated against corrosion.

Uniform non-porous surface for easy maintenance and hygiene.

Good resistance to chemical products and cleaning. Anti-UV treatment.

Warm to the touch.

Fixed by a 304 stainless steel plate, 4mm thick.

Supplied with stainless steel screws for concrete walls.

Dimensions: 650 x 230 x 105mm, Ø 32mm.

Tested to over 200kg. Maximum recommended user weight 135kg.

30-year warranty. CE marked.