**White L-shaped anti-bacterial Nylon shower grab bar, H. 750mm**

Bright white NylonClean anti-bacterial HR Nylon

Ø 32mm

Reference: **5070N**

Specification description

L-shaped shower grab bar Ø 32mm, for people with reduced mobility.

Helps the user stand and secures movement in the bath or shower.

Can be used as a shower rail by adding a shower head holder and/or soap dish.

NylonClean anti-bacterial treatment: optimal protection against bacterial development.

Dimensions: 750 x 450mm.

Can be installed with the upright to the left or right side.

Suitable for intensive use in public places or the healthcare sector.

High strength polyamide (Nylon): with 2mm reinforced steel core treated against corrosion.

Uniform non-porous surface for easy maintenance and hygiene.

Good resistance to chemical products and cleaning. Anti-UV treatment.

Warm to the touch.

38mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

Fixings concealed by a 6-hole cover plate, Ø 73mm.

Supplied with stainless steel screws for concrete walls.