**Wall-mounted toilet brush set with lid**

Model with anti-theft lock for fixing

White powder-coated 304 stainless steel

Reference: **4051EW**

Specification description

Wall-mounted toilet brush set with lid.

Wall-mounted, robust model with toilet brush with anti-theft lock for fixing.

Bacteriostatic white powder-coated 304 stainless steel.

Easy to clean: plastic bowl can be removed from above.

Plastic bowl with reservoir: avoids toilet brush sitting in residual water and reduces the risk of splashing when next used.

Toilet brush automatically centres itself in the holder.

Stainless steel body 1mm thick.

Dimensions: Ø 90 x 410mm.

30-year warranty.