**Hand dryer automatically activated by optical cell, with 360° nozzle**

Optical cell

304 bright polished stainless steel

Reference: **6613D**

Specification description

Automatic hand dryer.

Vandal-resistant model.

Electrical hand dryer automatically activated via optical cell.

360° rotating nozzle.

Metal thickness: 1.2mm.

Cover 304 stainless steel, bright polished finish.

Dimensions: 210 x 280 x 220mm.

Weight: 3.5kg.

Power: 2,000W. 50-60Hz.

Airflow: 95 l/second.

Low noise level: 68 dBA.

Maximum safety, Class II insulation(double electrical insulation), IP23.

CE marked, TÜV GS.

3-year warranty.