**Straight curtain rail**

Cut-to-size

Length 1m

Reference: **2359**

Specification description

Cut-to-size shower curtain rail.

Concealed fixings.

Rod for shower curtains made from bright polished 304 stainless steel tube, 1mm thick.

Dimensions: Ø 20mm, 1m can be cut to size.

30-year warranty.