**Straight curtain rail**

Cut-to-size

Length 2m

Reference: **4359**

Specification description

Cut-to-size straight shower curtain rail.

Concealed fixings.

Shower curtain rod made from bright polished 304 stainless steel tube, 1mm thick

Dimensions: Ø 20mm, 2m can be cut to size.

30-year warranty.