**BIOCLIP mechanical basin mixer**

Single hole removable mechanical mixer H.95mm L.120mm, solid lever

Pop-up waste and stopcocks

Reference: **2820T**

Specification description

Deck-mounted mechanical basin mixer.

BIOCLIP mechanical mixer: mixer can be removed entirely for cleaning and disinfection.

Single hole mixer with spout H. 95mm, L. 120mm fitted with a BIOSAFE hygienic flow straightener.

Ø 35mm ceramic cartridge with pre-set maximum temperature limiter.

Thermal shocks are easy to undertake without removing the control lever or shutting off the water supply.

Body and spout with smooth interiors and low water volume.

Flow rate limited to 5 lpm at 3 bar.

Solid control lever.

1 1/4" ergonomic pop-up waste made from brass.

PEX flexibles F3/8" supplied with stopcocks in chrome-plated brass.

Fixing reinforced by 2 stainless steel rods.

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Single hole mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.

Also available with copper tails