**Mechanical basin mixer**

Tall single hole, single control mixer with ceramic cartridge

Mixer with swivelling, removable spout

Reference: **2871T1**

Specification description

Deck-mounted tall mechanical basin mixer.

Single hole, single control with tall swivelling spout H. 180mm, L. 180mm.

Mechanical mixer supplied with 1 disposable, removable spout.

Ø 35mm ceramic cartridge with pre-set maximum temperature limiter.

Body and spout with smooth interiors (reduced bacterial development).

Thermal shocks are easy to undertake without removing the control lever or shutting off the cold water supply.

Flow rate regulated at 5 lpm at 3 bar.

Hygiene control lever L. 185mm for touch-free control.

Chrome-plated brass body and base.

F3/8" PEX flexibles .

Fixing reinforced by 2 stainless steel rods.

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Single control mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.