**Auto-draining shower kit with mechanical mixer**

Shower kit with wall-mounted single control mixer

With standard offset connectors

Reference: **2739SHYG**

Specification description

Shower kit with wall-mounted single control mechanical mixer.

Shower kit with auto-draining device.

• Wall-mounted single control mixer with Securitouch thermal insulation to prevent burns.

Ø 40mm classic ceramic cartridge with pre-set maximum temperature limiter.

Body with smooth interior and low water volume.

Flow rate regulated at 9 lpm.

Chrome-plated brass body and sculptured control lever.

M1/2" shower outlet with integrated non-return valve.

Mixer with offset standard wall connectors, M1/2" M3/4".

• Chrome-plated shower head (ref. 813) with flexible shower hose (836T3) and chrome-plated, adjustable, wall-mounted support (ref. 845).

• Auto-draining device FM1/2" for installation between the flexible hose and the shower head automatically drains the shower head and flexible hose (ref. 880).

Mixer is ideal for healthcare facilities, retirement homes, hospitals and clinics.

Mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.