**Auto-draining shower kit with mechanical mixer**

Mechanical mixer

With offset STOP/CHECK connectors

Reference: **2539HYG**

Specification description

Mechanical shower kit with auto-draining device:

 • Shower mixer with Ø 40mm ceramic cartridge with pre-set maximum temperature limiter.

 Flow rate regulated at 9 lpm.

Chrome-plated brass body and sculptured control lever.

M1/2" shower outlet with integrated non-return valve.

 Supplied with offset STOP/CHECK connectors, M1/2" M3/4", ideal for hospitals.

 • Shower head (ref. 813) with flexible hose (ref. 834T3) and chrome-plated, adjustable, wall-mounted support (ref. 845).

• Auto-draining device FM1/2" for installation between the flexible hose and the shower head, automatically drains the shower head and flexible hose (reduces bacterial development) (ref. 880).

30-year warranty.