**Stainless steel flexible shower hose**

Double interlock flexible hose FF1/2"

L. 1.50m

Reference: **832T1**

Specification description

Brass flexible shower hose, FF1/2", L. 1.50m.

Double interlock stainless steel for intensive use with non-twist connector at showe outlet

Food-grade, PVC inner tube conforms to European standard EN 1113.

Chrome-plated conical brass connectors 1/2".

Will withstand strain up to 50kg and twisting and bending.