**Twin hole pillar-mounted mixer - 100 lpm**

On pillar mounts

For plunge sinks

Reference: **5603**

Specification description

Twin hole mixer, M3/4" with 150mm centres on pillar mounts for plunge sinks.

Swivelling, tubular spout Ø 22mm H. 380mm L. 300mm.

Star-shaped, brass flow straightener.

Water-free, guided valve heads with reinforced mechanisms.

Shock-resistant ergonomic ball levers.

Flow rate 100 lpm at 3 bar suitable for plunge sinks.

Full flow rate within the first 90°.

Spout with smooth interior.

One-piece body and spout in chrome-plated brass.

Reinforced fixings and recessed inlets.

 30-year warranty.