**TEMPOSTOP 2 time flow tap**

Time flow tap

Reference: **702000**

Specification description

Deck-mounted time flow basin tap:

Time flow ~7 seconds.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Scale-resistant flow straightener.

Chrome-plated brass body M½".

Fixing with back-nut.

30-year warranty.