**TEMPOSTOP 2 time flow tap**

Lever-operated

Reference: **702400**

Specification description

Deck-mounted time flow lever-operated basin tap:

Time flow ~7 seconds.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Tamperproof scale-resistant flow straightener.

Solid chrome-plated brass body M½".

Fixing reinforced by back-nut with 3 stainless steel screws.

Lever control (soft-touch operation).

Suitable for people with reduced mobility.

30-year warranty.