**TEMPOSTOP time flow tap**

(AB) Anti-blocking model

Wall-mounted, ½"

Reference: **746001**

Specification description

TEMPOSTOP wall-mounted time flow basin tap:

Time flow ~7 seconds.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Tamperproof, scale-resistant flow straightener.

Chrome-plated brass body M½".

AB anti-blocking system: water will flow only when the push-button is released.

30-year warranty.