**Fixed spout**

L. 75mm

For panel over 30mm

Reference: **942040**

Specification description

Cross wall spout L. 75mm, M1/2".

For panels ≤ 30mm with anti-rotating pin.

Threaded rod can be cut-to-size.

Streamlined ligature-resistant design.

Chrome-plated solid brass.

Star-shaped scale-resistant flow straightener.

30-year warranty.