**TEMPOSOFT time flow shower panel**

Time flow, top inlet

Fixed shower head, aluminium

Reference: **749300**

Specification description

Time flow shower panel:

Anodised aluminium shower panel for wall-mounted, exposed installation.

TEMPOSOFT time flow shower valve for mixed water supply.

Soft-touch operation.

Time flow ~30 seconds.

Flow rate 6 lpm at 3 bar.

Chrome-plated, tamperproof, scale-resistant, fixed, ROUND shower head with automatic flow rate regulation.

Top inlet via in-line stopcock.

M½" mixed water connection.

Concealed fixings.

Filter.

Shower panel suitable for people with reduced mobility.

30-year warranty.