**TEMPOSOFT 2 time flow shower kit**

Time flow

Exposed, TONIC JET head

Reference: **747801**

Specification description

Time flow shower kit for exposed installation:

TEMPOSOFT 2 M½" time flow valve for mixed water supply from beneath.

For wall-mounted installation.

Soft-touch operation.

Time flow ~30 seconds.

Flow rate 6 lpm at 3 bar.

Chrome-plated, tamperproof TONIC JET shower head with scale-resistant nozzle and automatic flow rate regulation.

Chrome-plated solid brass.

Reinforced shower column Ø 16mm and collar (mounting bracket and screws supplied).

Suitable for people with reduced mobility.

30-year warranty.