**TEMPOSTOP time flow shower valve**

Time flow

For panels

Reference: **749770**

Specification description

Time flow shower valve for panels:

TEMPOSTOP M3/4" time flow valve for mixed water supply.

For panel mounting, 2mm max.

Chrome-plated metal wall plate Ø 70mm.

Time flow ~30 seconds.

Flow rate 12 lpm at 3 bar, can be adjusted.

Solid brass body and push-button.

Rear locking ring.

30-year warranty.