**ROUND shower head**

Scale-resistant

For panels from 1 to 15mm

Reference: **709010**

Specification description

Fixed shower head:

For installation on panels from 1 - 15mm.

Flow rate 6 lpm at 3 bar.

Automatic flow rate regulation.

Scale-resistant and ligature-resistant adjustable nozzle.

Chrome-plated solid brass.

Fixed with concealed blocking screw.

Systematically drains after use (no water retention or impurity deposits).

Inlets M½".

30-year warranty.