**TEMPOMATIC multi-urinals urinal valve**

Mains supply, electronic with barrier

Recessed

Reference: **487620**

Specification description

Recessed electronic valve with infrared barrier for urinals:

Rinsing for 1 - 8 urinals (standard or stall) or 2 siphon action urinals.

For recessed installation.

Electronic unit with 230/12V transformer.

Hydraulic unit with solenoid valve, stopcock M¾" and filter.

Hygienic duty flush every 24 hours after last use, prevents vacuums in the siphon.

Presence detection by infrared barrier.

Recessed Infrared detector Ø 50mm and reflector Ø 85mm.

Automatic pre-rinse possible after the arrival of the first user.

Automatic rinse every 30 or 60 sec.

Time flow pre-set at 3 sec., can be adjusted from 2 to 14 sec.

Flow rate 0.3 l/sec. at 3 bar pressure, can be adjusted.

Maximum detection range recommended: 6 meters.

Anti-blocking security: automatic shut-off after 20 uninterrupted cycles.

Suitable for people with reduced mobility.

30-year warranty.