**TEMPOSTOP time flow urinal valve**

Time flow 7 seconds

Recessed, with stainless steel wall plate

Reference: **779128**

Specification description

Recessed time flow urinal valve:

For standard or siphon action urinals.

For recessed installation.

Recessing depth can be adjusted from 25 to 40mm.

Stainless steel wall plate Ø 130mm.

Compatible with rain water.

Time flow ~7 seconds.

Flow rate pre-set at 0.25 l/sec. at 3 bar, can be adjusted.

Solid brass body F½".

30-year warranty.

This model does not have a waterproof recessing box. The installer must ensure that the recessing area is waterproof and any leaks or condensates can drain away (see installation guide).