**TEMPOSTOP time flow urinal valve**

Time flow 7 seconds

Recessed with satin st steel plate, F1/2"

Reference: **779427**

Specification description

Recessed time flow urinal valve:

For standard or siphon action urinals.

Recessed installation.

Recessing depth can be adjusted 25 - 45mm.

Stainless steel cover plate 160 x 160mm.

Compatible with rain water.

Time flow ~7 seconds.

Flow rate pre-set at 0.25 L/sec. at 3 bar, can be adjusted.

Solid brass body F½".

30-year warranty.

This model does not have a waterproof recessing housing. The installer must ensure that the recessing area is waterproof and any leaks or condensates can drain away (see installation guide).