**SIPHURINOIR**

Siphon with vertical outlet

Chrome-plated ABS

Reference: **771000**

Specification description

Urinal vertical siphon Ø 50mm with lip seal..

Outlet Ø 32mm with nut.

Water level 50mm.

Chrome-plated ABS.

30-year warranty.