**TEMPOFLUX 1 direct flush valve**

Direct flush WC valve

Recessed behind wall plate Ø 195mm

Reference: **761900**

Specification description

Flush system without cistern: directly connected to pipework.

Chrome-plated brass wall plate Ø 195mm.

Multipurpose recessing housing.

Soft-touch operation.

Time flow ~7 seconds.

Vacuum breaker.

Integrated stopcock and flow/volume rate adjuster.

Solid brass body and chrome-plated push-button.

In-line inlet M¾".

Outlet connection for PVC tube Ø 25mm.

Base flow rate: 1 L/sec.

30-year warranty.

This model does not have a waterproof recessing housing. The installer must ensure that the recessing area is waterproofand any leaks or condensation can drain away (see installation guide).