**TEMPOFLUX 1 direct flush kit**

Time flow direct flush WC kit

Exposed, 28mm tube, no stopcock

Reference: **761004**

Specification description

Flush system without cistern: directly connected to pipework.

Wall-mounted, exposed operation.

Soft-touch operation.

Time flow ~7 sec.

Vacuum breaker.

Chrome-plated solid brass body and push-button.

Inlet M¾".

With chrome-plated outlet tube, collar and connection washer.

Upstream supply pipes: minimum Ø 20mm required at all points (including connectors).

Base flow rate: 1 L/sec at 1 bar dynamic pressure.

Compatible with rain water.

Suitable for people with reduced mobility.

30-year warranty.