**TEMPOFLUX 1 direct flush valve**

Direct flush WC valve

Exposed, no stopcock

Reference: **761000**

Specification description

Flush system without cistern: directly connected to pipework.

For wall-mounted, exposed installation.

Soft-touch operation.

Time flow ~7 seconds.

Vacuum breaker.

Chrome-plated solid brass body and push-button.

Angled inlet M¾".

With outlet nut Ø 28mm.

Base flow rate: 1 L/sec at 1 bar dynamic pressure.

Compatible with rain water.

Suitable for people with reduced mobility.

30-year warranty.