**TEMPOCHASSE direct flush valve**

Time flow direct flush WC valve

Recessed, Time flow

Reference: **760220**

Specification description

Flush system without cistern: directly connected to pipework.

Satin finish stainless steel plate 320 x 220mm.

Time flow ~7 seconds.

Vacuum breaker.

In-line raw brass stopcock and flow rate / flush volume adjuster.

Solid brass body and chrome-plated metal push-button.

Shockproof mechanism.

In-line inlet F1".

Connection washer Ø 32/55mm.

Base flow rate: 1 L/sec at 1 bar dynamic pressure.

Compatible with rain water.

30-year warranty.

This model does not have a waterproof recessing housing. The installer must ensure that the recessing area is waterproof and any leaks or condensation can drain away (see installation guide).