**TEMPOCHASSE direct flush kit**

Time flow direct flush WC kit

Exposed, with in-line stopcock

Reference: **760004**

Specification description

Flush system without cistern: directly connected to pipework.

For wall-mounted exposed installation.

For conventional pans.

Time flow ~7 seconds.

Vacuum breaker.

In-line F1" chrome-plated brass stopcock and flow/volume rate adjuster.

Chrome-plated solid brass body and push-button.

Shock-resistant mechanism.

Bright polished stainless steel elbow flush tube Ø 32mm with nut and collar.

Base flow rate: 1 L/sec at 1 bar dynamic pressure.

Compatible with rain water.

30-year warranty.