**Shower kit with thermostatic mixer**

Shower riser rail with thermostatic mixer with no non-return valve

With standard connectors

Reference: **H9630SKIT**

Specification description

Shower riser kit with thermostatic sequential mixer,

Shower riser rail with SECURITHERM thermostatic shower mixer.

Thermostatic sequential mixer: opens and closes with cold water.

Mixer with no non-return valves on the inlets (reduces bacterial proliferation).

No risk of cross flow between hot and cold water.

Sequential mixer with anti-scalding failsafe: shuts off automatically if cold or hot water supply fails.

Securitouch thermal insulation prevents burns.

Scale-resistant, thermostatic sequential cartridge.

Temperature control from cold water up to 39°C with maximum temperature limiter set at 39°C.

Thermal shocks are possible.

Body with smooth interior and low water volume.

Flow rate regulated at 9 lpm.

Chrome plated brass body and Hygiene lever L. 100mm.

M1/2" bottom shower outlet.

Wall-mounted mixer with offset standard connectors M1/2" M3/4".

Mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

• Sliding shower head (ref. 813) on a chrome plated riser rail (ref. 821) with soap dish and flexible hose (ref. 836T1).

• Shower hose retaining collar (ref. 830).

Suitable for people with reduced mobility.

30-year warranty.