**TEMPOMIX time flow shower mixer**

Single control time flow

For panels 1- 10mm, Chrome-pltd Bayblend® control

Reference: **790970**

Specification description

Exposed time flow shower mixer:

TEMPOMIX ¾" single control mixer.

For panels 1 - 10mm.

Temperature control and operation via the push-button.

Maximum temperature limiter (can be adjusted by the installer).

Soft-touch operation.

Time flow ~30 seconds.

Flow rate 12 lpm at 3 bar, can be adjusted.

Chrome-plated solid brass.

Integrated non-return valves and filters.

Chrome-plated metal push-button.

30-year warranty.