**TEMPOSTOP**

For hand washbasins

Without button

Reference: **748126**

Specification description

Time flow ~7 seconds.

Flow rate pre-set at 3 lpm at 3 bar, adjustable from 1.5 to 6 lpm.

Rough cast brass body.

Inlet M½".

To be placed behind hand washbasin wall plate.

30-year warranty.