**BINOPTIC electronic tap**

Mains supply, Ø 15mm conical inlets

Recessed, spout with smooth interior

Reference: **379ENC15**

Specification description

Recessed electronic basin tap:

Independent IP65 electronic control unit.

230/12V mains supply with transformer.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Scale-resistant flow straightener.

Duty flush (pre-set flush ~60 seconds every 24 hours after last use).

Active, infrared movement detection, sensor at the end of the spout optimises detection.

Filter, solenoid valve and Ø 15mm conical inlet.

Chrome-plated solid brass body.

Chrome-plated spout L. 200mm for recessed installation.

Anti-blocking security.

Spout with a smooth interior and low water volume (limits bacterial niches).

30-year warranty.