**Lift-up Comfort shower seat**

Wall-mounted lift-up shower seat

UltraSatin polished satin stainless steel

Reference: **510420S**

Specification description

HR Comfort lift-up shower seat.

Wall-mounted, lift-up shower seat for fixed installation.

Shower seat for disabled people and for people with reduced mobility.

Large model.

Anti-bacterial treatment on the seat: optimal protection against bacterial development and mould.

Retained in upright position. Slowed down descent.

Suitable for intensive use in public places or the healthcare sector.

Removable solid seat made from high strength polymer.

Uniform non-porous surface for easy maintenance and hygiene.

Good resistance to chemical products (Betadine®) and cleaning.

Anti-UV treatment.

Warm to the touch.

Bacteriostatic 304 stainless steel structure Ø 32mm.

UltraSatin polished satin finish.

Concealed fixings secured to wall by a 304 stainless steel plate, 4mm thick.

Supplied with stainless steel screws for concrete walls.

Dimensions: 506 x 420 x 138mm.

Folded dimensions: 95 x 540mm.

Tested to over 200kg. Maximum recommended user weight: 135kg.

Lift-up shower seat with 30-year warranty. CE marked.