**Aluminium shower panel with SECURITHERM sequential mixer**

Sequential thermostatic mixer

Top inlets, shower head, aluminium, copper inlets

Reference: **H963915**

Specification description

SECURITHERM anodised aluminium shower panel for wall-mounted exposed installation:

 SECURITHERM sequential thermostatic mixer (non time flow).

 Temperature control from cold water up to 39°C.

 Maximum temperature limiter set at 39°C, can be adjusted.

 Anti-scalding failsafe: automatic shut-off if cold or hot water supply fails.

Thermal shocks are possible.

 Chrome-plated, tamperproof, scale-resistant ROUND shower head with automatic flow rate regulation at 6 lpm at 3 bar.

 Hygiene control lever L. 100mm.

 Top inlets with M1/2" stopcocks.

 With copper tails.

 Concealed fixings and filters.

30-year warranty.