**SECURITHERM shower panel**

Electronic battery-operated thermostatic

Concealed inlet, fixed head, aluminium

Reference: **792410UK**

Specification description

Electronic thermostatic shower panel:

Anodised aluminium shower panel for wall-mounted, exposed installation.

Concealed inlets via flexibles M½".

SECURITHERM thermostatic shower mixer.

Adjustable temperature control from cold water up to 38°C: 1st limiter set at 38°C, 2nd limiter set at 41°C.

Anti-scalding safety: immediate shut-off if cold or hot water supply fails.

Thermal shocks are possible.

Battery-operated with CR-P2 223 6V Lithium battery.

Infrared presence detection. Shower starts when hand is 4cm from the sensor.

Shuts off voluntarily or automatically after ~60 seconds.

Duty flush (~60 seconds every 24 hours after the last use).

Flow rate 6 lpm at 3 bar.

Chrome-plated, tamperproof, scale-resistant, fixed, ROUND shower head with automatic flow rate regulation.

Concealed fixings.

Filters and non-return valves.

Electronic shower panel suitable for people with reduced mobility.

30-year warranty.