**TRIPLO RP wall-mounted multiple washbasin**

Polished satin 304 stainless steel - L. 1800mm - With splashback

Without tap hole

Reference: **120750**

Specification description

Wash trough for wall-mounting, for 3 services, 1,800 x 500mm.

With an upstand to protect the wall from splashing and improve hygiene.

Basin internal diameter: 310mm.

Bacteriostatic 304 stainless steel.

Polished satin stainless steel.

Stainless steel thickness: 1.5mm

Rounded edges prevent injury.

With no tap hole.

Supplied with x3 1¼" wastes.

Without overflow.

Supplied with brackets and fixing elements.

CE marked. Complies with European standard EN 14688.

Weight: 22kg.

30-year warranty.

[Formerly ref: 0211750015]