**GENOU wall-mounted hand washbasin**

Polished satin 304 stainless steel - knee-operated

Tap included

Reference: **180330**

Specification description

Wall-mounted, knee-operated hand washbasin.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.2mm

Rounded edges prevent injury.

Supplied with swan neck spout and time flowtap with 7 second time flow.

Supplied with 1 ¼" waste.

Without overflow.

Supplied with fixing elements.

CE marked. Complies with European standard EN 14688.

Weight: 5kg.

30-year warranty.

[Formerly ref: 0211030003]