**SHA XS squat WC pan**

Polished satin 304 stainless steel - recessed - no trap

1 spreader

Reference: **113710**

Specification description

Floor-recessed squat WC pan, 500 x 220 x 600mm.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness 1.2mm.

One-piece pressed WC bowl, seam-free for easy maintenance and better hygiene.

Bowl shape suitable for male and female use.

Non-slip foot area.

Waste outlet: Ø 100mm.

Flushing system with one 304 stainless steel spreader.

Weight: 5kg.

30-year warranty.

[Formerly ref: 0113370019]