**L trough urinal**

Polished satin 304 stainless steel - L. 1,800mm - Floor-recessed

Reference: **130220**

Specification description

Floor-standing recessed trough urinal, 1800 x 1020 x 300mm.

Bacteriostatic 304 stainless steel.

Stainless steel thickness: 1.2mm.

Rear water inlet.

Supplied with 3 stainless steel rinsers and 3 flexible hoses.

Water saving: optimal rinsing with 0.1 L/sec. per service i.e. 0.3L per use.

Central drainage.

Waste outlet 1½". Supplied with waste and integrated trap (ref. 785000).

Weight: 34kg.

Possible to add one or more bacteriostatic 304 stainless steel dividers. Fix directly onto the urinal in the desired location.