**TU urinal divider for wall-mounting**

Polished satin 304 stainless steel - H. 700mm

Reference: **100610**

Specification description

Urinal divider for wall-mounting.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.5mm

Smooth surface and rounded edges.

Supplied with theft prevention TORX security screws.

Weight: 6.2kg.

[Formerly ref: 0011610000]