**Pressure-balancing mixer with retracting hand spray**

Single hole mechanical EP mixer with retracting hand spray

Mixer with Hygiene control lever

Reference: **2211LEP**

Specification description

Deck-mounted mechanical sink mixer with pressure-balancing suitable for baby baths.

Single hole mixer with retracting hand spray with swivelling spout H. 105mm L. 200mm.

Ø 40mm ceramic cartridge with pressure-balancing and pre-set maximum temperature limiter.

Total anti-scalding safety: HW flow rate is reduced if CW supply fails (and vice versa).

Stable temperature regardless of variations in pressure and flow rate.

Securitouch thermal insulation prevents burns.

Mechanical mixer with retracting hand spray with 2 jet options: flow straightener / rain effect.

Body with smooth interior.

Flow rate 7 lpm at 3 bar.

Chrome-plated brass body and Hygiene control lever.

BIOSAFE flexible shower hose reduces bacterial proliferation: transparent polyurethane flexible hose ensures replacement if biofilm is present, smooth interior and exterior.

Narrow flexible (interior Ø 6mm), low water volume.

Specific counterweight.

F⅜" PEX flexibles with filters and non-return valves.

Fixing reinforced by 2 stainless steel rods.

SECURITHERM mechanical mixer with pressure-balancing ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Single hole mixer suitable for people with reduced mobility.

30-year warranty.