**Wall-hung BCN S WC pan**

Dual finish 304 stainless steel

Reference: **110112**

Specification description

Wall-hung WC pan, 360 x 340 x 550mm.

Compatible with all standard frame systems available on the market.

Elegant and simple design.

Bacteriostatic 304 stainless steel.

Dual finish: bright polished pan interior and polished satin exterior.

Stainless steel thickness: 1.5mm.

WC bowl surface is polished with rounded edges for easy cleaning.

Concealed perimetral flushing rim.

Horizontal water inlet: Ø 55mm.

Horizontal waste outlet: Ø 100mm.

Water saving: works with 4L or more of water.

Pre-drilled holes for fixing the toilet seat. Supplied with stainless steel blanking caps when installed without toilet seat lid.

Quick and easy to install from the front thanks to a stainless steel mounting frame.

Supplied with fixing plate and 6 theft prevention TORX security screws.

CE marked. Complies with European standard EN 997 for 4L flush.

30-year warranty.

Weight: 12kg.