**Securitouch mechanical shower mixer**

Wall-mounted single control mixer, solid lever

With offset standard connectors

Reference: **2739TS**

Specification description

Wall-mounted single control mechanical shower mixer.

Wall-mounted single control mixer with Securitouch thermal insulation to prevent burns.

Ø 40mm classic ceramic cartridge with pre-set maximum temperature limiter.

Body with smooth interior and low water volume.

Flow rate regulated at 9 lpm.

Chrome-plated brass body and solid control lever.

M1/2" shower outlet with integrated non-return valve.

Mixer with offset standard connectors M1/2" M3/4".

Shower mixer ideal for healthcare facilities, nursing homes, hospitals and clinics.

Shower mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.