**TEMPOMATIC 4 electronic tap**

Recessed mains supply

Recessed, L. 130mm, integrated electronics

Reference: **443400**

Specification description

Wall-mounted electronic basin tap:

230/6V recessed mains supply.

Reduced-stagnation solenoid valve and electronic unit integrated into the body of the tap.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 - 6 lpm.

Scale-resistant flow straightener.

Duty flush (~60 seconds every 24 hours after last use).

Presence detection sensor at the end of the spout optimises detection.

Chrome-plated stainless steel body L. 130mm.

Cap fixed in place by 2 concealed screws.

Stopcock.

Wall-mounted fixings.

Recessed inlet.

Anti-blocking security.

Suitable for people with reduced mobility.

30-year warranty.